****************************************************************************
** ENU *********************************************************************
****************************************************************************
*                                                           
*  Intel(R) Chipset Software Installation Utility
*  Installation Readme
*                                                           
*  NOTE:  This document refers to systems containing the 
*               following Intel chipsets: 
* 
*               Intel(R) 810  Chipset
*               Intel(R) 810E Chipset
*               Intel(R) 815  Chipset
*               Intel(R) 815E Chipset
*               Intel(R) 815EM Chipset
*               Intel(R) 820  Chipset
*               Intel(R) 820E Chipset
*               Intel(R) 840  Chipset
*               Intel(R) 850  Chipset
*               Intel(R) 440BX AGPset
*               Intel(R) 440DX AGPset
*               Intel(R) 440EX AGPset
*               Intel(R) 440GX AGPset
*               Intel(R) 440LX AGPset
*               Intel(R) 440ZX AGPset
*               Intel(R) 440MX Chipset
*               Intel(R) 430TX PCIset
*               Intel(R) 815EP Chipset
*               Intel(R) 810E2 Chipset
*
*
****************************************************************************
****************************************************************************


****************************************************************************
*  CONTENTS OF THIS DOCUMENT
****************************************************************************
This document contains the following sections:

1.  Overview
2.  System Requirements
3.  Installing the Software
    3A. Installing the Software in Interactive Mode
    3B. Installing the Software in Silent Mode
    3C. List of Available Command Line Flag Options
4.  Verifying Installation of the Software
5.  Contents of the Distribution Package
6.  Identifying the Software Version Number
7.  Troubleshooting

****************************************************************************
* 1.  OVERVIEW
****************************************************************************
The Intel(R) Chipset Software Installation Utility installs
to the target system the Windows* INF files that outline to 
the operating system how the chipset components will be 
configured.  This is needed for the proper functioning of
the following features:

   - Core PCI and ISAPNP Services
   - AGP Support
   - IDE/ATA33/ATA66 Storage Support
   - USB Support
   - Identification of Intel Chipset Components in 
     Device Manager

****************************************************************************
* 2.  SYSTEM REQUIREMENTS 
****************************************************************************
1.  The software included with this distribution package is 
     designed to operate with the following chipset 
     configurations:

               Intel(R) 810  Chipset
               Intel(R) 810E Chipset
               Intel(R) 815  Chipset
               Intel(R) 815E Chipset
               Intel(R) 815EM Chipset
               Intel(R) 820  Chipset
               Intel(R) 820E Chipset
               Intel(R) 840  Chipset
               Intel(R) 850  Chipset
               Intel(R) 440BX AGPset
               Intel(R) 440DX AGPset
               Intel(R) 440EX AGPset
               Intel(R) 440GX AGPset
               Intel(R) 440LX AGPset
               Intel(R) 440ZX AGPset
               Intel(R) 440MX Chipset
               Intel(R) 430TX PCIset
               Intel(R) 815EP Chipset
               Intel(R) 810E2 Chipset

              
2.  One of the following operating systems must be 
    installed on the system:
    Windows 95      4.00.950   (Original release)
    Windows 95      4.00.950a  (OSR1)
    Windows 95      4.00.950b  (OSR2 without USB 
                                Supplement)
    Windows 95      4.00.950b  (OSR2.1 with USB 
                                Supplement)
    Windows 95      4.00.950c  (OSR2.5 with or 
                                without USB Supplement)
    Windows 98      4.10.1998  (Original release)
    Windows 98 Second Edition
                              4.10.2222  (Original release)         
    Windows ME     4.90.3000  (Original release)
    Windows 2000  5.00.2195  (Original release)

To verify which operating system has been installed onto 
the target system, follow the steps below:

    a.  Click on Start.
    b.  Select Settings.
    c.  Select Control Panel.
    d.  Double-click on the System icon.
    e.  Click on the General system properties tab.
     f.  Verify which OS has been installed by reading
         the System information.
                              
3.  The software should be installed on systems with at
     least 32 MB of system memory.

4.  There should be sufficient hard disk space in the <TEMP>
     directory (typically C:\WINDOWS\TEMP) of the system on
     which this software is installed.

Please check with your system provider to determine which 
operating system and Intel chipset are used in your system.  

****************************************************************************
* 3.  INSTALLING THE SOFTWARE 
****************************************************************************
This software can be installed in two modes: Interactive or 
Silent.  The Interactive Mode requires user input during
installation; the Silent Mode does not.

Additionally, this software offers a set of command line
flag options that enable extended installation functionality.
The command line flags are not case-sensitive.  See Section 
3C for detailed descriptions of these flags.

Important Note:
The Intel(R) Chipset Software Installation Utility is 
distributed in two formats -- self extracting .EXE files
(INFINST_xxx.EXE) or compressed .ZIP files (INFINST_xxx.ZIP).  
Depending on which distribution format is being executed, 
the command-line syntax may differ.  See Section 3C for more
details.

****************************************************************************
* 3A.  INSTALLING THE SOFTWARE IN INTERACTIVE MODE
****************************************************************************
1.  Check the System Requirements.  The operating system 
     must be fully installed and running on the system before
     running this software.

2.  Close any running applications.  Otherwise, you may
     experience difficulties.

3.  Run the InstallShield* installation program:
       Self-extracting .EXE distribution: INFINST_xxx.EXE
       Compressed .ZIP distribution     : SETUP.EXE

4.  You will be prompted to agree to the license agreement.  
     If you do not agree, the Installer will exit before 
     extracting any files.
    
5.  Follow the on-screen instructions and use the default
     settings to complete the setup, once the operating
     system has rebooted.

6.  This completes the installation of the Intel(R) Chipset 
     Software Installation Utility.  

****************************************************************************
* 3B.  INSTALLING THE SOFTWARE IN SILENT MODE
****************************************************************************
1.  Check the System Requirements.  The operating system 
     must be fully installed and running on the system before 
     running this software.

2.  Close any running applications.  Otherwise, you may 
     experience difficulties.

3.  Run the InstallShield installation program:
     For silent install with auto-reboot:
       Self-extracting .EXE distribution:
                                    INFINST_xxx.EXE -a -b -s
       Compressed .ZIP distribution     : 
                                    SETUP.EXE -b -s
    - OR -
     For silent install without auto-reboot:
       Self-extracting .EXE distribution: 
                                    INFINST_xxx.EXE -a -s
       Compressed .ZIP distribution     :
                                    SETUP.EXE -s

4.  The utility will perform the necessary updates and 
     record the installation status in the following 
     system registry key:
        HKEY_LOCAL_MACHINE\Software\Intel\INFInst

5.  If the utility was invoked with the "-b" flag, the 
     system will automatically reboot if the update was
     successful.

    NOTE:  The system MUST be rebooted for all device 
                 updates to take effect.

6.  To determine whether the install was successful,
     verify the 'install' value in the registry key
     specified in Step 4.

     The following table describes the various parameter 
     values:

     Value      Type      Data        Description
     ------     ----      ----        -----------
    "install"   String  "success"     The installation
                                       was successful.
                        "fail"        The installation 
                                       was not successful.
                                       No INF files were 
                                       copied to the 
                                       system.                

    "reboot"  String     "Yes"        A reboot is required
                                       to complete the 
                                       installation.
                         "No"         No reboot is required
                                       to complete the 
                                       installation.
                                
    "version" String    <varies>      Current version 
                                       number of the 
                                       Intel(R) Chipset 
                                       Software Installation
                                       Utility
                                         
****************************************************************************
* 3C.  LIST OF AVAILABLE COMMAND LINE FLAG OPTIONS
****************************************************************************
The Intel(R) Chipset Software Installation Utility supports  
several command line flags for various installation options. 
All command line flags and parameters must be separated by a 
space, except for the language code after the '-L' flag.

Due to the different distribution formats available for the
Intel(R) Chipset Software Installation Utility, the command
line flag syntax may vary:

1. Self-Extracting .EXE Distribution:
      When installing this software using the .EXE 
      distribution, an extra '-A' must be appended to the 
      INFINST_xxx.EXE program call (i.e. INFINST_ENU.EXE -A)
      in order to successfully pass command line parameters.
      The extra '-A' flag for the self-extracting .EXE 
      package is DIFFERENT from the '-A' command line flag
      option described below.  

      Example: To extract INF files using the '-A' flag 
                     described below, the installation program 
                     should be invoked as follows:  
          
               INFINST_ENU.EXE -A -A (optional -P)

2. Compressed .ZIP Distribution:
      When installing this software using the .ZIP 
      distribution, there is no need to append any extra 
      flags to the SETUP.EXE program call in order to pass
      command line flags.

      Example: To extract INF files using the '-A' flag 
                     described below, the installation program 
                     should be invoked as follows:  
                        
               SETUP.EXE -A (optional -P)

Below is a list of all the available command line flags 
that may be used with the program call.  Note that the
'-L' and the '-S' flags MUST be specified at the end of 
the command line flag list.

Flag         Description
----            -----------
-?             Help flag.  Displays the list of available
                command line flags.  This parameter works 
                in the Interactive mode only.  

-A             Extracts INF files, README.TXT  and 
                instructions for OEM preload (PRELOAD.TXT) 
                to either "C:\Program Files\Intel\InfInst" 
                or the <Installation Path> directory 
                specified using the '-P' flag.  The 
                software will NOT install these INF files 
                to the system.  This flag can be combined 
                only with the '-P' flag option.  All other 
                options will be ignored if the '-A' flag 
                is specified. This parameter works in 
                either Silent mode or Interactive mode.

-B             Automatically reboots the system after 
                installation.  This flag is ignored if '-A'
                flag is specified.  This parameter works 
                in either Silent mode or Interactive mode.

-L<LangCode>   
                Forces the InstallShield user interface to 
                display the specified language during 
                setup.  Note that there should be NO 
                spaces between '-L' and the 4-digit 
                language code (see below).  This flag and 
                the '-S' flag must be placed at the end 
                of the command line flag list.  This 
                parameter works in Interactive mode only.

-P <Installation Path>   
                Specifies the HDD location to which the
                INF program files are copied.  If this 
                flag is not specified at the command line,
                the <Installation Path> directory is by 
                default assumed to be:
                
                   C:\Program Files\Intel\INFInst
                
                If this flag is used without the '-A' 
                option, only README.TXT  will be copied to
                <Installation Path>.  The directory name 
                can include spaces.  In this case, 
                however, a pair of double quotes (") must
                enclose the directory name.  This 
                parameter works in either Silent mode or
                Interactive mode.

-S             Runs the Installer in silent mode.  No 
                user interface is displayed.   This flag
                and the '-L' flag must be placed at the
                end of the command line flag list.

                
Below are the language codes used with the '-L' flag:

    Language                          <LangCode>
    --------                          ----------
    Chinese (PRC)                     0804
    Chinese (Taiwan)                  0404
    Danish                            0006
    Dutch                             0013
    English (UK - International)      0809
    English (US)                      0409
    Finnish                           000B
    French (Canadian)                 0C0C
    French (Standard)                 040C
    German                            0007
    Italian                           0010
    Japanese                          0011
    Korean                            0012
    Norwegian                         0014
    Polish                            0015
    Portuguese (Brazilian)            0416
    Portuguese (Standard)             0816
    Russian                           0019
    Spanish                           000A
    Swedish                           001D
    Thai                              001E

****************************************************************************
* 4.  VERIFYING INSTALLATION OF THE SOFTWARE
****************************************************************************
Run Device Manager to verify the correct installation and
usage of the INF files.

For Windows 95, Windows 98 and Windows 98 Second Edition,
Windows ME:

   1.  Click on Start.
   2.  Select Settings.
   3.  Select Control Panel.
   4.  Double-click on System icon.
   5.  Click on Device Manager tab.
   6.  Click on View Devices by Connection button.
   7.  Click on Plug and Play BIOS, or Advanced
        Configuration and Power Interface (ACPI) BIOS.
   8.  Click on PCI bus.

For Windows 2000:

   1.  Click on Start.
   2.  Select Settings.
   3.  Select Control Panel.
   4.  Double-click on System icon.
   5.  Click on Hardware tab.
   6.  Click on Device Manager button.
   7.  From the View menu, select menu item Devices by
        connection.
   8.  Click on Standard PC, or
        Advanced Configuration and Power Interface (ACPI)
        PC.
   9.  Click on PCI bus.

After the Device Manager is launched as described above,
check the descriptions for the following entries:

    *** NOTE:  Device Manager will display only the names
                      of devices currently detected in the 
                      system.

    Intel(R) 810 Chipset:
        Intel(R) 82810 System and Graphics Controller 
        -or-
        Intel(R) 82810 DC-100 System and Graphics 
           Controller
  
    Intel(R) 810E Chipset, Intel(R) 810E2 Chipset:
        Intel(R) 82810E DC-133 System and Graphics 
           Controller 

    Intel(R) 820 Chipset, Intel(R) 820E Chipset:
        Intel(R) 82820 Processor to I/O Controller
        Intel(R) 82820 Processor to AGP Controller

    Intel(R) 840 Chipset:
        Intel(R) 82840 Processor to I/O Controller 
        Intel(R) 82840 Processor to AGP Controller 
        Intel(R) 82840 PCI Bridge 
              
     Intel(R) 82806AA PCI 64-bit Hub:
        Intel(R) 82806AA Advanced Programmable Interrupt
           Controller
        Intel(R) 82806AA PCI Bridge
        Intel(R) 82806AA Controller (reserved)

    Intel(R) 82801AA I/O Controller Hub (ICH):
        Intel(R) 82801AA LPC Interface Controller 
        Intel(R) 82801AA Ultra ATA Controller 
        Intel(R) 82801AA USB Universal Host Controller 
        Intel(R) 82801AA SMBus Controller 
        Intel(R) 82801AA PCI Bridge 
      
    Intel(R) 82801AB I/O Controller Hub (ICH0):
        Intel(R) 82801AB LPC Interface Controller 
        Intel(R) 82801AB Ultra ATA Controller 
        Intel(R) 82801AB USB Universal Host Controller 
        Intel(R) 82801AB SMBus Controller 
        Intel(R) 82801AB PCI Bridge 

    Intel(R) 82371AB PCI to ISA/IDE Xcelerator (PIIX4):
        Intel(R) 82371AB PCI to ISA bridge (EIO mode)
        Intel(R) 82371AB PCI to ISA bridge (ISA mode)
        Intel(R) 82371AB Power Management Controller
        Intel(R) 82371AB/EB/MB PCI Bus Master IDE 
           Controller
        Intel(R) 82371AB/EB/MB PCI to USB Universal Host
           Controller
   
    Intel(R) 82371EB/MB PCI to ISA/IDE Xcelerator (PIIX4):
        Intel(R) 82371EB/MB PCI to ISA bridge (EIO mode)
        Intel(R) 82371EB/MB PCI to ISA bridge (ISA mode)
        Intel(R) 82371EB/MB Power Management Controller
        Intel(R) 82371AB/EB/MB PCI Bus Master IDE 
           Controller
        Intel(R) 82371AB/EB/MB PCI to USB Universal Host 
           Controller

    Intel(R) 82371SB PCI to ISA/IDE Xcelerator (PIIX3):
        Intel(R) 82371SB PCI to ISA bridge
        Intel(R) 82371SB PCI Bus Master IDE Controller
        Intel(R) 82371SB PCI to USB Universal Host
           Controller    

    Intel(R) 440MX Chipset:
        Intel(R) 82440MX Processor to I/O Controller
        Intel(R) 82440MX PCI to ISA Bridge
        Intel(R) 82440MX Power Management Controller
        Intel(R) 82440MX Bus Master IDE Controller
        Intel(R) 82440MX USB Universal Host Controller

    Intel(R) 430TX PCIset:
        Intel(R) 82443TX Processor to PCI bridge

    Intel(R) 440BX AGPset, Intel(R) 440DX AGPset, 
      Intel(R) 440ZX AGPset:
        Intel(R) 82443BX/ZX/DX Processor to PCI bridge
        Intel(R) 82443BX/ZX/DX Processor to AGP controller

    Intel(R) 440GX AGPset:
        Intel(R) 82443GX Processor to PCI bridge
        Intel(R) 82443GX Processor to AGP controller

    Intel(R) 440LX AGPset:
        Intel(R) 82443LX Processor to PCI bridge
        Intel(R) 82443LX Processor to AGP controller

    Intel(R) 815 Chipset, Intel(R) 815E Chipset, Intel(R) 815EP Chipset,
      Intel(R) 815EM Chipset:
        Intel(R) 82815 Processor to I/O Controller - 1130 
        Intel(R) 82815 Processor to AGP Controller - 1131 

    Intel(R) 82801BA I/O Controller Hub:
        Intel(R) 82801BA LPC Interface Controller - 2440 
        Intel(R) 82801BA PCI Bridge - 244E 
        Intel(R) 82801BA Ultra ATA Storage 
           Controller - 244B 
        Intel(R) 82801BA/BAM SMBus Controller - 2443 
        Intel(R) 82801BA/BAM USB Universal Host 
           Controller - 2442 
        Intel(R) 82801BA/BAM USB Universal Host 
           Controller - 2444 
        Intel(R) 82801BA/BAM AC '97 Audio Controller - 2445 

    Intel(R) 82801BAM I/O Controller Hub:
        Intel(R) 82801BAM LPC Interface Controller - 244C
        Intel(R) 82801BAM PCI Bridge - 2448
        Intel(R) 82801BAM Ultra ATA Storage 
           Controller - 244A
        Intel(R) 82801BA/BAM SMBus Controller - 2443 
        Intel(R) 82801BA/BAM USB Universal Host 
           Controller - 2442 
        Intel(R) 82801BA/BAM USB Universal Host 
           Controller - 2444 
        Intel(R) 82801BA/BAM AC '97 Audio 
           Controller - 2445 

    Intel(R) 850 Chipset:
        Intel(R) 82850 Processor to I/O Controller - 2530
        Intel(R) 82850/82860 Processor to AGP 
           Controller - 2532

 

10. On certain systems, the following device may also be 
      updated:
 
     a. Click on View Devices by Connection button.
     b. Click on Plug & Play BIOS, or Advanced 
         Configuration and Power Interface (ACPI) BIOS.     
     c. Verify that the following entry is present:
         Intel(R) 82802 Firmware Hub Device -OR-
         Intel(R) Security Driver

****************************************************************************
* 5.  CONTENTS OF THE DISTRIBUTION PACKAGE
****************************************************************************
The Intel(R) Chipset Software Installation Utility package 
contains the following items:

    File(s)       
    -------
    INFINST_xxx.EXE -or- INFINST_xxx.ZIP
    README.TXT

The version of the software included in the distribution
package is specified in the file RELNOTES.TXT.  

RELNOTES.TXT is available in English only.

After installation on a Windows 95, Windows 98, Windows ME or
Windows 2000 system, one or more of the following 
INF files are copied to the <Windows>\INF directory:

    File(s)
    -------
    440MXCOR.INF
    440MXIDE.INF
    440MXUSB.INF
    810.INF
    810B.INF
    820.INF
    820B.INF
    840.INF
    850.INF
    ICH2AUD.INF
    ICH2CORE.INF
    ICH2IDE.INF
    ICH2SMB.INF
    ICH2USB.INF
    ICHx.INF
    ICHxIDE.INF
    ICHxSMB.INF
    ICHxUSB.INF
    IFWH.INF
    IHOST.INF
    P64H.INF
    P64HRES.INF
    PIIXXIDE.INF
    PIIXXUSB.INF
    PIIX4.INF
    815.INF
    ICH2CORM.INF
    ICH2IDEM.INF


   *** NOTE:  Only the files that reference the currently 
                     detected devices are copied to the system.
                     If the -A option is exercised, the files are
                     not copied to the <Windows>\INF directory.
                     See Section 3C for more information.

One or more of the following digital signature files are 
installed to the <Windows>\CATROOT directory on a 
Windows 98, Windows ME or Windows 2000 system ONLY:

    File(s)
    -------
    440MXCOR.CAT
    440MXIDE.CAT
    440MXUSB.CAT
    810.CAT
    820.CAT
    820B.CAT
    840.CAT
    850.CAT
    ICHx.CAT
    ICHxIDE.CAT
    ICHxSMB.CAT
    ICHxUSB.CAT
    IFWH.CAT
    P64H.CAT
    P64HRES.CAT
    815.CAT
    ICH2AUD.CAT
    ICH2CORE.CAT
    ICH2IDE.CAT
    ICH2USB.CAT
    ICH2SMB.CAT
    ICH2CORM.CAT
    ICH2IDEM.CAT


   *** NOTE:  Only the files that reference the currently 
                     detected devices are copied to the system.
                     If the -A option is exercised, the files are
                     not copied to the <Windows>\CATROOT directory.
                     See Section 3C for more information.              

****************************************************************************
* 6.  IDENTIFYING THE SOFTWARE VERSION NUMBER
****************************************************************************
The version of the software included in the distribution
package is specified in the file RELNOTES.TXT.  

RELNOTES.TXT is available in English only.

The version of the software included in the distribution 
package can also be identified by examining the following 
registry location:

    Key name:   \\HKEY_LOCAL_MACHINE\Software\Intel\InfInst
    Value name: version

****************************************************************************
* 7.  TROUBLESHOOTING
****************************************************************************
It is assumed that the system requirements in Section 2 
above have been satisfied.

Issue:      System locks up during Device Manager Remove or 
               during restart.

Solution:  System lockup can occur during Restart as a 
                result of several possible system issues.  In 
                the event of system lockup, restart the machine 
                and view Device Manager.  If devices are listed 
                properly and the system experiences no further 
                problems, then the .INF file restore process was 
                successful.  If devices are not configured 
                correctly, try re-running the procedures 
                outlined in Section 3.

               If this does not fix problems or further 
               problems are experienced, reinstall the 
               operating system.


Issue:      After running the setup program and rebooting 
               the machine, Windows reports that it cannot 
               find one of the following files:
                  ESDI_506.pdr

Solution:  Click Browse in the dialog box where this 
                problem occurs, locate the

                  <Windows>\System\IOSubsys

                directory and click OK.  The system should
                be able to locate this file in this directory 
                and continue re-enumerating for the new 
                devices.

Issue:       After running the setup program and rebooting
                the machine, Windows reports that it cannot 
                find one of the following files:
 
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   Click Browse in the dialog box where this 
                 problem occurs, locate the

              <Windows>\System32\drivers (for Windows 98,
                              Windows ME)
               -or-
             
              <Windows>\System           (for Windows 95)

                 directory, and click OK.  The system should
                 be able to locate this file in this directory 
                 and continue re-enumerating for the new 
                 devices.

Issue:      During setup, installation stops and prompts 
               for one of the following files:
      
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   Ensure that the Windows 95 USB Supplement has 
                 been installed prior to running the Intel(R)
                 Chipset Software Installation Utility setup 
                 program.

Issue:       After running the setup program and rebooting
                the machine, Windows reports that it cannot 
                find the following file:
                  isapnp.vxd

Solution:   Click Browse in the dialog box where this 
                 problem occurs, locate the
 
                  <Windows>\System

                directory, and click OK.  The system should
                be able to locate this file in this directory 
                and continue re-enumerating for the new 
                devices.

Issue:      After performing the silent install, the 
               HKLM\Software\Intel\InfInst key was not created 
               or the data of the value "install" is not 
               "success".

Solution:   This is caused by one of the following 
                 scenarios:
               - The current system does not contain 
                 a supported operating system, or
               - The current system does not contain 
                 a supported chipset.

                Verify the System Requirements in Section 2.

****************************************************************************
****************************************************************************
* DISCLAIMER
****************************************************************************
Intel is making no claims of usability, efficacy or 
warranty.  
The INTEL SOFTWARE LICENSE AGREEMENT
(OEM / IHV / ISV Distribution & Single User) 
completely defines the licensed use of this software.
****************************************************************************
Information in this document is provided in connection with 
Intel products.  No license, express or implied, by estoppel 
or otherwise, to any intellectual property rights is granted 
by this document.  Intel assumes no liability whatsoever, 
and Intel disclaims any express or implied warranty 
relating to sale and/or use of Intel products, including 
liability or warranties relating to fitness for a particular 
purpose, merchantability or infringement of any patent, 
copyright or other intellectual property right.  Intel 
products are not intended for use in medical, life saving, 
or life-sustaining applications.

****************************************************************************
Intel Corporation disclaims all warranties and liabilities 
for the use of this document and the information contained 
herein, and assumes no responsibility for any errors which 
may appear in this document, nor does Intel make a 
commitment to update the information contained herein.  Intel 
reserves the right to make changes to this document at any 
time, without notice.
****************************************************************************
****************************************************************************

* Third-party brands and names are the property of their 
respective owners.

Copyright (c) Intel Corporation, 1997-2000

